# Sequence model for preparation for and clean-up of operation

Draping of robot arms and camera and placement of arms (sweet spot). Including focusing, calibration and heating of the optics

Measuring and placement of ports (10 cm from each other)

Docking of the robot

Insertion of instruments

Operation ( tool changing)

End of operation

Cleaning instruments

De-docking

Drapes removed

System shut down