# Sequence model for preparation and clean-up of operation

Draping of robot arms and camera and placement of arms (sweet spot). Including focusing, calibration and heating of the optics

Measuring and placement of ports

Docking of the robot

Insertion of instruments

Operation

End of operation

Cleaning instruments

De-docking

Drapes removed

System shut down